For 1990-2009 cars

### Removal Procedure

1. Disengage the 2 plastic snaps which secure the luggage compartment carpet to the floor at the rear of the luggage compartment.
2. Remove 4 plastic retaining clips along the forward edge of the luggage compartment floor.
3. Lift the carpet over the rear seat back in order to gain access to the rear seat back outboard hinges.
4. Place the rear seat back in the folded position.
5. Remove the 4 screws (1) which secure the rear seat back to the outboard hinges.
6. Remove the rear seat back, with the attached carpet, from the vehicle.

### Installation Procedure

1. Install the rear seat back to the vehicle. Secure the rear seat back to the outboard hinges with the 4 screws (1).
2. Place the seat back in the upright position.
3. Position the luggage compartment carpet into place and secure with the following:

• | 4 plastic retaining clips along the forward edge of the luggage compartment floor.

• | 2 plastic snaps at the rear of the luggage compartment.