For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disconnect the audio alarm module electrical connector.
3. Slide the audio alarm module (1) off of the retaining bracket.
4. Remove the audio alarm module (1) from the vehicle.

### Installation Procedure

1. Slide the audio alarm module (1) onto the retaining bracket.
2. Connect the audio alarm module electrical connector.
3. Connect the negative battery cable.