For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Backup Lamp Switch (Manual Transaxle) | Left side of the engine compartment, on top of the transaxle | Lighting Systems Component Views | Lighting Systems Connector End Views
Center High-Mounted Stoplamp (CHMSL) | Bottom of the rear window | -- | Lighting Systems Connector End Views
Daytime Running Lamps (DRL) Control Module | Behind the left side of the IP | Lighting Systems Component Views | Lighting Systems Connector End Views
Diode Module | Behind the center IP, taped to the IP harness | Lighting Systems Component Views | Engine Controls Connector End Views in Engine Controls
Illumination Controller | In the IP, left of the steering column | -- | Lighting Systems Connector End Views
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
LH Front Door Jamb Switch | Frame of the left front door, in the lower rear of the corner | Lighting Systems Component Views | --
Luggage Compartment Lamp (4-Door) | Center of the luggage compartment, under the rear window shelf | Lighting Systems Component Views | Lighting Systems Connector End Views
Luggage Compartment Lamp Switch (4-Door) | Center rear of the luggage compartment, mounted to the striker of the deck lid | -- | --
Park Brake Switch | Passenger compartment, behind the manual selector | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Radio | Center of the IP | -- | Entertainment Connector End Views in Entertainment
Rear Defogger Switch | In the IP, to the left of the steering column | -- | Stationary Windows Connector End Views in Stationary Windows
Rear Wiper/Washer Switch (2-Door LSi) | In the IP, to the left of the steering column | -- | Wiper/Washer Connector End Views in Wipers/Washer Systems
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Stoplamp Switch | Top of the brake pedal | Lighting Systems Component Views | Lighting Systems Connector End Views
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to the top of the transaxle | -- | Automatic Transmission Connector End Views in Automatic Transmission
Turn Signal/Combination Switch | On the steering column | -- | Lighting Systems Connector End Views
C112 (16 Cavities) | Main harness to the engine harness, on the right rear side of the engine compartment, near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (14 Cavities) | Main harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (13 Cavities) | IP harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C207 (3 Cavities) | IP harness to the dome lamp harness, on the right side of the upper cowl | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (10 Cavities) (4-Door) | Floor harness to the harness of the luggage compartment, on the left front side of the luggage compartment, near the left rear speaker | Harness Routing Views in Wiring Systems | --
C402 (6 Cavities) (2-Door) | Floor harness to the lift-gate harness, in the right rear corner | Harness Routing Views in Wiring Systems | --
G102 | Left front side of the engine compartment, on the inside of the left front fender, near the battery | Harness Routing Views in Wiring Systems | --
G103 | Right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views in Wiring Systems | --
G201 | Behind the left side of the knee bolster | Harness Routing Views in Wiring Systems | --
G202 | Right side of the center IP, behind the radio | Harness Routing Views in Wiring Systems | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G400 (2-Door) | Rear center of the luggage compartment | Harness Routing Views in Wiring Systems | --
(4-Door) | Rear center of the luggage compartment | Harness Routing Views in Wiring Systems | --
G401 (2-Door) | Center of the liftgate, near the rear wiper motor | Harness Routing Views in Wiring Systems | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P400 | Left rear side of the luggage compartment | -- | --
P401 | Right rear of the luggage compartment | -- | --
P402 | Center rear side of the luggage compartment | Harness Routing Views in Wiring Systems | --
P403 (2-Door) | Upper right side of the liftgate | Harness Routing Views in Wiring Systems | --
S100 | Main harness, approximately 10 cm (4 in) from the breakout of G103 | Harness Routing Views in Wiring Systems | --
S102 | Main harness, approximately 8 cm (3.1 in) from the breakout of G102 | Harness Routing Views in Wiring Systems | --
S104 | Main harness, approximately 13 cm (5.1 in) from the breakout of the brake fluid level switch | Harness Routing Views in Wiring Systems | --
S105 | Main Harness, approximately 6 cm (2.4 in) from the breakout of the Relay Box | Harness Routing Views in Wiring Systems | --
S107 | Main Harness, approximately 22 cm (8.8 in) from P200 | Harness Routing Views in Wiring Systems | --
S113 | Main harness, approximately 6 cm (2.4 in) from the G102 breakout | Harness Routing Views in Wiring Systems | --
S117 | Main harness, at the G103 breakout | Harness Routing Views in Wiring Systems | --
S154 (Automatic Transaxle) | Engine Harness, approximately 9 cm (3.6 in) from P202 | Harness Routing Views in Wiring Systems | --
S162 | Engine harness, approximately 10 cm (4 in) from P202 | Harness Routing Views in Wiring Systems | --
S202 | Main harness, approximately 8 cm (3.125 in) from the breakout of connector C6 of the junction block | -- | --
S204 | Main harness, approximately 8 cm (3.125 in) from the breakout of connector C5 of the junction block | -- | --
S205 | Main harness, approximately 1 cm (0.375 in) from P200 | -- | --
S206 (With ABS) | Main harness, approximately 22 cm (9 in) from the stoplamp switch connector breakout | -- | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S209 | Main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | Main harness, approximately 15 cm (6 in) from C208 | -- | --
S217 | IP harness, at the C200 breakout | Harness Routing Views in Wiring Systems | --
S218 | IP harness, approximately 3 cm (1.19 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S219 | IP Harness, approximately 3 cm (1.19 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S221 | IP harness, approximately 7 cm (3 in) from the breakout of IP cluster assembly connector C2 | Harness Routing Views in Wiring Systems | --
S222 | IP harness, approximately 6 cm (2.375 in) from the breakout of the data link connector | Harness Routing Views in Wiring Systems | --
S223 | Main harness, approximately 10 cm (4 in) from P200 | -- | --
S228 | IP harness, at the C200 breakout | Harness Routing Views in Wiring Systems | --
S229 | IP harness, approximately 4 cm (2 in) from the breakout of the IP cluster assembly connector C1 | Harness Routing Views in Wiring Systems | --
S230 | IP harness, approximately 13 cm (5.125 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S236 | IP harness, approximately 8 cm (3.125 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S238 | IP harness, approximately 3 cm (1.19 in) from the breakout of the blower motor connector | Harness Routing Views in Wiring Systems | --
S239 | IP harness, approximately 11 cm (4.313 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S241 | IP harness, approximately 5 cm (2 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S242 | IP harness, at the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S243 | IP harness, approximately 5 cm (2 in) from the breakout of the cigar lighter connector | Harness Routing Views in Wiring Systems | --
S244 | Main harness, approximately 23 cm (9.06 in) from P200 | -- | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S248 | Engine harness, approximately 4 cm (2 in) from the breakout of powertrain control module (PCM) connector C1 | Harness Routing Views in Wiring Systems | --
S250 | IP harness, approximately 6 cm (2.375 in) from the breakout of the diode module connector | Harness Routing Views in Wiring Systems | --
S252 | IP harness, approximately 4 cm (2 in) from the breakout of the data link connector | Harness Routing Views in Wiring Systems | --
S254 | IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views in Wiring Systems | --
S256 | Main harness, near the breakout of connector C6 of the junction block | -- | --
S302 | Floor harness, approximately 10 cm (4 in) from the C201 breakout | Harness Routing Views in Wiring Systems | --
S310 (4-Door) | Floor harness, approximately 6 cm (2.375 in) from the breakout of connector C8 of the junction block | Harness Routing Views in Wiring Systems | --
S400 (2-Door) | Floor harness, approximately 36 cm (14.17 in) from the C402 breakout | -- | --
(4-Door) | Floor harness, approximately 39 cm (14.19 in) from the connector breakout of the left rear combination lamp | -- | --
S401 (2-Door) | Floor harness, approximately 13 cm (5.125 in) from the G400 breakout | -- | --
(4-Door) | Floor harness, approximately 27 cm (11 in) from the connector breakout of the left rear combination lamp | -- | --
S402 (2-Door) | Floor harness, approximately 5 cm (2 in) from the connector breakout of the left rear combination lamp | -- | --
S403 (2-Door) | Floor Harness, approximately 5 cm (2 in) from the G400 breakout | -- | --
S404 (2-Door) | Floor harness, approximately 8 cm (3.125 in) from the G400 breakout | -- | --
(4-Door) | Floor harness, approximately 10 cm (4 in) from the connector breakout of the lamp switch in the luggage compartment | -- | --
S405 (2-Door) | Floor harness, approximately 13 cm (5.125 in) from the connector breakout of the left rear combination lamp | -- | --
(4-Door) | Floor harness, approximately 34 cm (13.375 in) from the connector breakout of the left rear combination lamp | -- | --
S406 (4-Door) | Floor harness, approximately 10 cm (4 in) from the connector breakout of the left rear combination lamp | -- | --
S407 (4-Door) | Floor harness, approximately 20 cm (8 in) from the connector breakout of the left rear combination lamp | -- | --
S408 (4-Door) | Floor harness, approximately 5 cm (2 in) from the C400 breakout | -- | --
S410 (2-Door) | Pigtail of the right rear combination lamp, approximately 8 cm (3.125 in) from P401 | -- | --
S411 | Pigtail of the right rear combination lamp, approximately 6 cm (2.375 in) from P401 | -- | --
S412 (2-Door) | Pigtail of the left rear combination lamp, approximately 8 cm (3.125 in) from P400 | -- | --
S413 | Pigtail of the left rear combination lamp, approximately 6 cm (2.375 in) from P400 | -- | --
S419 (4-Door) | Floor harness, approximately 21 cm (8.25 in) from the connector breakout of the left rear door jamb switch | -- | --