For 1990-2009 cars

2. Install the transaxle range switch (714) onto the manual shift shaft (7086).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the transaxle range switch retaining bolt.

Tighten
Tighten the transaxle range switch retaining bolt to 23 N·m (17 lb ft).

4. Install the transaxle range switch harness retaining clamps to the transaxle case.

Tighten
Tighten the range switch harness retaining clamp bolts to 23 N·m (17 lb ft).