For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Pull the water deflector far enough away from the door in order to gain access to the inside door handle (4).
3. Remove the 2 screws and the inside door handle (4) from the door.
4. Remove the following components from the inside door handle (4):

• | The handle rod

• | The handle lock rod

### Installation Procedure

1. Install the following components to the inside door handle (4):

• | The handle rod

• | The handle lock rod

2. Install the inside door handle (4) to the door. Secure the handle with the 2 screws.
3. Apply adhesive to the back of the water deflector.
4. Place the water deflector in its normal position.
5. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .