For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Left side of engine compartment | Power and Grounding Component Views | --
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views | --
Fuse Box | Left side of the engine compartment, mounted on Left inner side of the fender, behind the relay box | Power and Grounding Component Views | Power and Grounding Connector End Views
Generator | Right rear side of the engine compartment, mounted to the engine | Engine Electrical Component Views | --
Ignition Switch | Right side of the steering column | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views in Engine Controls - 1.0L or Engine Controls Component Views in Engine Controls - 1.3L | Powertrain Control Module Connector End Views in Engine Controls - 1.0L or Powertrain Control Module Connector End Views in Engine Controls - 1.3L
Starter Motor | Center rear of engine | Engine Electrical Component Views | --
Starter Solenoid | Center rear of engine, top of the starter motor | Engine Electrical Component Views | --
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to top of the transaxle | -- | Automatic Transmission Connector End Views
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views | Inline Harness Connector End Views
C113 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near the bulkhead | Harness Routing Views | Inline Harness Connector End Views
C204 (2 Cavities) (Manual Transaxle) | Main harness to clutch pedal position switch, behind left side of the IP | Harness Routing Views | --
C205 (12 Cavities) | IP harness to engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views | Inline Harness Connector End Views
G100 | Mounted on top of the left side of the transaxle | -- | --
G101 | Left front side of the engine compartment, front of the battery | -- | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views | --
S101 | Main harness, approximately 11 cm (4.5 in) from the brake fluid level switch breakout | Harness Routing Views | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views | --
S160 (VIN 2) | Engine Harness, approximately 20 cm (8 in) from P202 | -- | --
S162 | Engine harness, approximately 10 cm (4 in) from P202 | Harness Routing Views | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S231 | Main harness, approximately 15 (6 in) cm from P200 | -- | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views | --