For 1990-2009 cars

### Removal Procedure

1. Remove the A/C compressor control module (2) from the evaporator case by performing the following actions:

• | Unsnap the module (2)

• | Slide the module (2) up.

2. Disconnect the electrical connector of the A/C compressor control module .
3. Remove the A/C compressor control module from the vehicle.

### Installation Procedure

1. Install the A/C compressor control module (2) to the vehicle.
2. Connect the electrical connector of the A/C compressor control module .
3. Install the A/C compressor control module to the evaporator case. Slide and snap the A/C compressor control module into place.