For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Cut the hog rings on the bottom of the seat cushion.

Important: The top of the cover is bonded to the seat's foam pad. Remove the cover carefully.

3. Remove the seat cushion cover.

### Installation Procedure

1. Install the seat cushion cover to the seat cushion.
2. Bond the seat cushion cover to the top of the cushion with 3M general trim adhesive, or equivalent.
3. Using hog ring pliers, secure the cover to the seat cushion with the new hog rings.
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .