For 1990-2009 cars

All automatic transaxle equipped models of this vehicle are equipped with steering columns that contain a mechanical neutral start system. This system relies on a mechanical block in order to prevent starting the engine with the transaxle in any position other than P (park) or N (neutral).

An interlink (back drive) cable connects the ignition switch to the gearshift selector. This cable prevents the gearshift selector from moving unless the ignition is in the ON position. Refer to the appropriate procedure in Automatic Transaxle for further service information.