For 1990-2009 cars

### Removal Procedure

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the 2 screws (1,7) which secure the composite headlamp/turn signal/parking lamp housing assembly (6).
3. Remove the bulb sockets from the housing assembly.
4. Remove the composite headlamp housing assembly from the vehicle.

### Installation Procedure

1. Install the bulb sockets to the housing assembly.
2. Install the composite headlamp/turn signal/parking lamp housing assembly (6) to the vehicle. Secure the assembly with the 2 screws (1,7).
3. Connect the negative battery cable.
4. Adjust the composite headlamp aim. Refer to Headlamp Aiming .