For 1990-2009 cars

## Rear Quarter Molding Replacement 2 Door

1. Wash the affected panel area with soap and water.
2. Wipe the area dry.
3. Remove all traces of adhesive from the following areas using oil-free naphtha or alcohol:

• | The body panel (3)

• | The back of the molding (2)

4. Mark the proper position of the molding (2) using a length of masking tape. Use the adjacent moldings as a guide, if applicable.
5. If the vehicle body is below 21°C (70°F) due to shop temperature or outside temperature, warm the body panel using a heat gun before proceeding.
6. Apply one of the following double-coated acrylic foam tapes to the molding (2):

• | P/N 06380, 3M Super Automotive Attachment Tape (which has a white backing)

• | P/N 06382 (which has a gray backing), or the equivalent

7. Align the molding (2) to the tape guideline.
8. Firmly press the molding (2) in place.

## Rear Quarter Molding Replacement 4 Door

1. Wash the affected panel area with soap and water.
2. Wipe the area dry.
3. Remove all traces of adhesive from the following areas using oil-free naphtha or alcohol:

• | The body panel (3)

• | The back of the molding

4. Mark the proper position of the molding using a length of masking tape. Use the adjacent moldings as a guide, if applicable.
5. If the vehicle body is below 21°C (70°F) due to shop temperature or outside temperature, warm the body panel (3) using a heat gun before proceeding.
6. Apply one of the following double-coated acrylic foam tapes to the molding:

• | P/N 06380, 3M Super Automotive Attachment Tape (which has a white backing)

• | P/N 06382 (which has a gray backing), or the equivalent

7. Align the molding to the tape guideline.
8. Firmly press the molding in place.