For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Pull the water deflector far enough away from the door in order to gain access to the inside door handle (4).
3. Remove the 2 screws and the inside door handle (4) from the door.
4. Remove the following components from the inside door handle (4):

• | The handle rod

• | The handle lock rod

### Installation Procedure

1. Install the following components to the inside door handle (4):

• | The handle rod

• | The handle lock rod

2. Install the inside door handle (4) to the door. Secure the handle with the 2 screws.
3. Apply adhesive to the back of the water deflector.
4. Place the water deflector in a normal position.
5. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .