For 1990-2009 cars

### Removal Procedure

1. Disconnect the 2 hoses from the EVAP canister air filter (1).
2. Remove the 2 bolts that attach the EVAP canister air filter (1) to the vehicle chassis.
3. Remove the EVAP canister air filter from the vehicle.

### Installation Procedure

1. Install the EVAP canister air filter to the vehicle chassis.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the two bolts that secure the EVAP canister air filter (1) to the chassis.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Connect the 2 hoses to the EVAP canister air filter (1), and secure the hoses with clamps.