For 1990-2009 cars

### Removal Procedure

1. Remove the nozzle seal from the nozzle (2).
2. Gently disengage the lock tabs of the nozzle. Pull the nozzle from the hatchback door.
3. Disconnect the washer hose (8) from the nozzle (2).

### Installation Procedure

1. Connect the washer hose (8) to the nozzle (2).
2. Install the nozzle to the hatchback door.
3. Install the nozzle seal to the nozzle (2).