For 1990-2009 cars

Name | Location
--- | ---
A/C Amplifier | Below right side of the IP, attached to evaporator case
Blower Speed Selector Switch | Center of IP, above radio
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal
Combination Switch on | Steering Column
Crankshaft Position Sensor | Bottom of the engine, mounted to the engine near the crankshaft pulley
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console
Diode Module | Behind the center IP, taped to the IP harness
Distributor | Left side of the engine
Duty Check Data Link Connector | Left Rear of the Engine Compartment Near the Shock Tower
Early Fuel Evaporation (EFE) Heater | Mounted between the intake manifold and the throttle body
Engine Coolant Temperature (ECT) Sensor | Left side of the engine, mounted in thermostat housing
Engine Cooling Fan Motor | Left front side of the engine compartment, behind the radiator
EVAP Canister Purge Valve | Right side engine compartment, on the intake manifold
Exhaust Gas Recirculation Vacuum Solenoid (EGR SV) Valve | Left side of the engine, next to the intake manifold
Exhaust Gas Recirculation (EGR) Bypass Valve | Left side of the engine, next to the intake manifold
Fuel Injector | In the engine throttle body
Fuel Injector Resistor | Left rear side of the engine compartment, attached to the bulkhead
Fuel Sender Assembly | In the fuel tank
Fuse Box | Left side of the engine compartment, mounted on Left inner side of the fender, behind the relay box
Heated Oxygen Sensor 1 (HO2S1) | Front of the engine in the exhaust manifold
Heated Oxygen Sensor 2 (HO2S2) | Below vehicle after a three-way catalytic converter (TWC)
Idle Speed Control (ISC) Motor | Top of engine, mounted to the throttle body
Ignition Control Module | Left engine compartment on the bulkhead near the strut tower
Ignition Coil | Left side of the engine compartment, on the bulkhead
Ignition Switch | Right side of the steering column
Instrument Panel Cluster Assembly | Left side of the IP
Intake Air Temperature (IAT) Sensor | Center engine compartment attached to air cleaner (ACL) housing
Junction Block | Behind left side of the IP
Manifold Absolute Pressure (MAP) Sensor | Right rear engine compartment, on the bulkhead
Noise Suppressor Filter | Left rear engine compartment, taped to the harness, below the ignition control module
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box
Rear Defogger Switch | In the IP, left of steering column
Relay Box | Left front engine compartment, near the battery
Throttle Position (TP) Sensor | Right rear side of the engine, attached to the throttle body
Turn Signal/Combination Switch | On steering column
Vehicle Speed Sensor (VSS) (Automatic Transaxle) | Left side of the engine compartment, top of the transaxle