For 1990-2009 cars

#### Tools Required

• | J 34839 Pinion Bearing Remover

• | J 37764 Pilot Bearing Remover Adapter

• | J 23907 Clutch Pilot Bearing Remover

• | J 36190 Drive Handle

• | J 34848 Clutch Pilot Bearing Installer

### Removal Procedure

1. Remove the manual transaxle assembly from the vehicle. Refer to Transaxle Assembly Removal in Manual Transmission.
2. Remove the clutch pressure plate. Refer to Clutch Assembly Replacement .
3. Remove the clutch disc. Refer to Clutch Assembly Replacement .
4. Use J 34839 , J 37764 and J 23907 in order to remove the clutch pilot bearing (1).
5. Inspect the clutch pilot bearing (1) for the following conditions:

• | Scoring

• | Binding

• | Damage

### Installation Procedure

1. Use J 34848 with J 36190 in order to install the clutch pilot bearing (1) into the crankshaft .
2. Install the clutch disc. Refer to Clutch Assembly Replacement .
3. Install the pressure plate. Refer to Clutch Assembly Replacement .
4. Install the manual transaxle assembly into the vehicle. Refer to Transaxle Assembly Installation in Manual Transmission.