For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement .
2. Remove the following components from the liftgate:

• | 3 screws

• | The lock (1)

### Installation Procedure

1. Install the lock (1) to the liftgate. Secure the lock with 3 screws.
2. Install the liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement .