For 1990-2009 cars

There are many different materials on the market used to repair tires. Manufacturers have published detailed instructions on how and when to repair tires. These instructions can be obtained from the tire manufacturer if the instructions are not included with the repair kit. Due to their shallow 3.2 mm (0.125 in) tread depth, tire repair of the temporary spare tire is not recommended.