For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (2) from the air cleaner cover.
2. Release the 2 retaining clips (1) from the air cleaner box to the air cleaner cover.
3. Swing the air cleaner cover to the side in order to remove the air filter element.

### Installation Procedure

1. Install the air filter element into the air cleaner box.
2. Align the air cleaner cover over the air cleaner box.Secure the cover with the 2 retaining clips (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the bolt (2) that retains the air cleaner cover to the inner fender.

Tighten
Tighten the bolt to 10 N·m (89 lb in).