For 1990-2009 cars

### Removal Procedure

1. Remove the IP center trim bezel. Refer to Instrument Panel Center Trim Panel Replacement .
2. Gently lift and push in the ashtray guide in order to separate the ashtray guide from the IP center trim bezel.

### Installation Procedure

1. Install the ashtray guide to the IP center trim bezel.
2. Install the IP center trim bezel. Refer to Instrument Panel Center Trim Panel Replacement .