For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Countershaft Nut | 70 N·m | 52 lb ft
Differential Ring Gear Bolts | 85 N·m | 63 lb ft
Gearshift Arm Bolt | 36 N·m | 26 lb ft
Gearshift Fork Plug | 13 N·m | 10 lb ft
Gearshift Guide Case Bolts | 10 N·m | 89 lb in
Gearshift Interlock Bolt Strength 7 Bolt | 23 N·m | 17 lb ft
Gearshift Interlock Bolt Strength 9 Bolt | 34 N·m | 25 lb ft
Gearshift Shaft Bolt | 13 N·m | 10 lb ft
Gearshift Shaft Screws | 13 N·m | 10 lb ft
Gearshift Yoke Bolt | 36 N·m | 26 lb ft
Left Case Cap Bolts | 10 N·m | 89 lb in
Left Case Plate Screws | 12 N·m | 8.5 lb ft
Oil Gutter Bolt | 12 N·m | 8.5 lb ft
Reverse Gearshift Lever Bolts | 23 N·m | 17 lb ft
Reverse Idler Shaft Bolt | 14 N·m | 10 lb ft
Speedometer Driven Gear Case Retaining Bolt | 6 N·m | 53 lb in
Transaxle Case Bolts | 22 N·m | 16 lb ft
Transaxle Side Cover Bolts | 6 N·m | 53 lb in

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 23 N·m | 17 lb ft
Clutch Cable Bracket Bolts | 28 N·m | 21 lb ft
Clutch Release Lever Bolt and Nut | 23 N·m | 17 lb ft
Extension Rod Retaining Nut | 40 N·m | 29 lb ft
Flywheel Cover Bolts | 20 N·m | 15 lb ft
Gearshift Control Lever Guide Plate Bolts | 10 N·m | 89 lb in
Gearshift Control Lever Housing Nuts | 6 N·m | 53 lb in
Gearshift Control Lever Housing-to-Guide Plate Nuts | 40 N·m | 29 lb ft
Gearshift Control Shaft Front Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Control Shaft Joint Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Control Shaft Rear Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Guide Case Bolts | 12 N·m | 106 lb in
Gearshift Interlock Bolt | 28 N·m | 21 lb ft
Gearshift Yoke Bolt | 28 N·m | 21 lb ft
Left Case Cover Bolts | 12 N·m | 106 lb in
Left Transaxle Mount Bracket Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Retaining Nuts | 60 N·m | 44 lb ft
Left Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Rear Transaxle Mount Retaining Bolts | 60 N·m | 44 lb ft
Rear Transaxle Mount Through Bolt and Nut | 60 N·m | 44 lb ft
Right Case-to-Engine Block Mounting Bolts | 60 N·m | 44 lb ft
Speedometer Driven Gear Case Retaining Bolt | 7 N·m | 62 lb in
Starter Motor Retaining Bolts | 28 N·m | 21 lb ft
Transaxle Drain Plug | 21 N·m | 15 lb ft
Transaxle Hanger Bolt | 12 N·m | 106 lb in
Transaxle Oil Lever/Filler Plug | 21 N·m | 15 lb ft
Transaxle Side Cover Bolts | 12 N·m | 106 lb in