For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the ON position.
2. Move the blower speed selector switch to the following positions in the following order:

2.1. | LOW

2.2. | M1

2.3. | M2

2.4. | HIGH

2.5. | LOW

• | The blower motor speed increases as the blower speed selector switch is moved toward the HIGH position.

• | The blower motor speed decreases as the blower speed selector switch is moved toward the LOW position.

• | Blower Motor Operates at High Speed Only

• | Blower Motor High Speed Inoperative

• | Blower Motor Inoperative Med-2

• | Blower Motor Inoperative Med-1

• | Blower Motor Low Speed Inoperative

• | Blower Motor Inoperative at Any Speed

• | Blower Motor Always On

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.