For 1990-2009 cars

### Removal Procedure

1. Gently pry-out the left vent garnish (5) with a small flat screwdriver from the IP.
2. Remove the IP center outlet duct. Refer to IP Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or HVAC Systems - Manual.
3. Remove the 2 screws and the left vent louver (6) from the IP.

### Installation Procedure

1. Install the left vent louver (6) to the IP. Secure the louver with the 2 screws.
2. Install the left vent garnish panel (5) to the IP. Push the panel in until the panel fully engages.
3. Install the IP center outlet duct. Refer to IP Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or HVAC Systems - Manual.