For 1990-2009 cars

### Removal Procedure

1. Remove the outer sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
2. Remove the rear door reveal molding (1) from the rear door by removing the 2 screws.

### Installation Procedure

1. Install the rear door reveal molding (1) to the rear door. Secure the molding with 2 screws.
2. Install the outer sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .