For 1990-2009 cars

## Ignition Coil Replacement 1.3L

### Removal Procedure

1. Disconnect the two spark plug wires from the 1-4 ignition coil (2) or the 2-3 ignition coil (1). Note the routing to ensure correct assembly.
2. Disconnect the ignition coil electrical connector.
3. Remove the two bolts and the ignition coil from the cylinder head.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the ignition coil to the cylinder head and secure with the two bolts.

Tighten
Tighten the ignition coil attaching bolts to 10 N·m (8 lb ft).

2. Connect the ignition coil electrical connector.
3. Connect the correct two spark plug wires to 1-4 ignition coil (2) or the 2-3 ignition coil (1).

## Ignition Coil Replacement 1.0L

### Removal Procedure

1. Remove the coil wire from the ignition coil.
2. Disconnect the ignition coil electrical connector.
3. Disconnect the ignition coil ground wire electrical connector.
4. Remove two bolts and the ignition coil mounting bracket (1) from the bulkhead.
5. Remove two screws and the ignition coil from the mounting bracket.

### Installation Procedure

1. Install the ignition coil to the ignition coil mounting bracket (1). Secure with two screws.
2. Install the ignition coil mounting bracket to the bulkhead. Secure with two bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the ignition coil mounting bracket bolts to 15 N·m (11 lb ft).

3. Connect the ignition coil ground wire electrical connector.
4. Connect the ignition coil electrical connector.
5. Connect the coil wire to the ignition coil.