For 1990-2009 cars

### Removal Procedure

1. Disconnect the fuel injector resistor electrical connector.
2. Remove the two bolts and the fuel injector resistor (1) with bracket from the engine compartment bulkhead.
3. Remove the two screws and the fuel injector resistor from the bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the fuel injector resistor to the bracket with the two screws.

Tighten
Tighten the fuel injector resistor attaching screws to 2.8 to 3.5 N·m (24 to 31 lb in).

2. Install the fuel injector resistor (1) and bracket to the engine compartment bulkhead with the two bolts.

Tighten
Tighten the fuel injector resistor bracket bolts to 10 N·m (89 lb in).

3. Connect the fuel injector resistor electrical connector.