For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster from the instrument panel. Refer to Instrument Cluster Replacement .

Important: Remember the location of the bulb sockets for proper installation.

3. Remove all of the bulb sockets from the back of the cluster assembly.
4. Remove the screws (1,2,3,4) from the back of the instrument cluster assembly.
5. Remove the printed circuit from the back of the instrument cluster assembly.

### Installation Procedure

1. Install the printed circuit to the back of the instrument cluster assembly. Secure the printed circuit with all of the gauge screws (1,2,3,4).
2. Install all of the bulb sockets to the back of the instrument cluster assembly.
3. Install the instrument cluster to the instrument panel. Refer to Instrument Cluster Replacement .
4. Connect the negative battery cable.