For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror. Refer to Manual Mirror Replacement .
2. Remove the screw that secures the outer sealing strip (7) to the door.
3. Unclip the plastic clips holding the outer sealing strip (7) to the door panel.

### Installation Procedure

1. Clip the outer sealing strip (7) into place on the door panel.
2. Install the screw that secures the outer sealing strip (7) to the door panel.
3. Install the outside rearview mirror. Refer to Manual Mirror Replacement .