For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .

Important: Remember the location of the bulb sockets (3,4) for proper installation.

2. Remove all of the bulb sockets (3,4) from the back of the cluster (6).
3. Remove the screws (1,2,3,4) from the back of the instrument cluster assembly.
4. Remove the printed circuit (1) from the back of the instrument cluster (6).

### Installation Procedure

1. Install the printed circuit (1) to the back of the instrument cluster (6).
2. Secure the printed circuit with all of the gauge screws (1,2,3,4).
3. Install all of the bulb sockets (3,4) to the back of the instrument cluster (6).
4. Install the instrument panel cluster. Refer to Instrument Cluster Replacement .