For 1990-2009 cars

### Removal Procedure

1. Disengage the 2 plastic snaps which secure the luggage compartment carpet to the floor at the rear of the luggage compartment.
2. Remove 4 plastic retaining clips along the forward edge of the luggage compartment floor.
3. Place the rear seat back (2) in the folded position.
4. Lift the carpet over the rear seat back (2) in order to gain access to the rear retaining clips which secure the rear seat cushion to the floor pan.
5. Remove 1 screw (1) from each rear retaining clip.
6. Raise the seat cushion at the front edge in order to disengage the front retaining clips.
7. Slide the seat cushion over the seat belt buckles.
8. Remove the seat cushion from the vehicle.

### Installation Procedure

1. Install the seat cushion in the vehicle.
2. Feed the seat belt buckles through the seat cushion.
3. Engage the front retaining clips in order to secure the seat cushion to the vehicle.
4. Secure each rear retaining clip to the floor pan with 1 screw (1).
5. Place the seat back (2) in the upright position.
6. Position the luggage compartment carpet into place and secure with the following:

• | 4 plastic retaining clips along the forward edge of the luggage compartment floor.

• | 2 plastic snaps at the rear of the luggage compartment.