For 1990-2009 cars

## Radio Rear Speaker Replacement 2-Door

### Removal Procedure

1. Remove the rear quarter trim panel. Refer to Rear Quarter Trim Panel Replacement in Interior Trim.
2. Disconnect the rear speaker electrical connector.
3. Remove the following components from the vehicle:

3.1. | 4 screws

3.2. | The rear speaker (1)

### Installation Procedure

1. Install the speaker (1) to the inner rear quarter panel. Secure the speaker with the 4 screws.
2. Connect the rear speaker electrical connector.
3. Install the rear quarter trim panel. Refer to Rear Quarter Trim Panel Replacement in Interior Trim.

## Radio Rear Speaker Replacement 4-Door

### Removal Procedure

1. Remove the seat back to rear window trim panel. Refer to Liftgate Trim Panel Replacement in Body Rear End.
2. Disconnect the rear speaker electrical connector.
3. Remove the following components from the vehicle:

3.1. | 4 screws

3.2. | The rear speaker (1)

### Installation Procedure

1. Install the rear speaker (1) to the rear seat back to the rear window shelf. Secure the speaker with the 4 screws.
2. Connect the rear speaker electrical connector.
3. Install the rear seat back to rear window trim panel. Refer to Liftgate Trim Panel Replacement in Body Rear End.