For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Blower Motor | Behind the right side of the IP | Heater Blower Controls Component Views | --
Blower Motor Resistor | Behind the right side of the IP in the blower assembly | Heater Blower Controls Component Views | --
Blower Speed Selector Switch | Center of IP, above radio | Heater Blower Controls Component Views | --
Junction Block | Behind left side of the IP | Data Link Communications Component Views in Wiring Systems | --
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C208 (8 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C211 (6 Cavities) | IP harness to blower speed selector switch jumper, behind the center of the IP | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G202 | Right side of the center IP behind the radio | Power and Grounding Component Views In Wiring Systems | --
S232 | IP harness, approximately 4 cm (2 in) from C204 breakout | Harness Routing Views in Wiring Systems | --
S233 | IP harness, approximately 8 cm (3.125 in) from the blower motor branch breakout | Harness Routing Views in Wiring Systems | --
S234 | IP harness, approximately 1 cm (.375 in) from the diode module connector breakout | Harness Routing Views in Wiring Systems | --
S238 | IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views in Wiring Systems | --
S243 | IP harness, approximately 5 cm (2 in) from the cigar lighter connector breakout | Harness Routing Views in Wiring Systems | --