For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the IP center trim bezel (4). Refer to Instrument Panel Center Trim Panel Replacement .
3. Remove the retaining ring (3) from the rear of the cigar lighter (6).
4. Remove the following components from the IP center trim bezel (4):

• | The front parts of the cigar lighter (6)

• | The rear parts of the cigar lighter (6)

• | The rim (5)

### Installation Procedure

1. Install the following components to the IP center trim bezel (4):

• | The front parts of the cigar lighter (6)

• | The rear parts of the cigar lighter (6)

• | The rim (5)

2. Install the retaining ring (3) to the rear of the cigar lighter (6).
3. Install the IP center trim bezel (4). Refer to Instrument Panel Center Trim Panel Replacement .
4. Connect the negative battery cable.