For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views | Data Link Communications Connector End Views
Electronic Brake Control Module (EBCM) (With ABS) | Behind the left IP, above the junction block | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Inflatable Restraint Sensing and Diagnostic Module (SDM) | The center of the console, in front of the manual selector | SIR Component Views in SIR | SIR Connector End Views inSIR
Junction Block | Behind the left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
C200 (12 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 (12 Cavities) | The IP harness to the engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (5 Cavities) | Supplemental inflatable restraint (SIR) harness to the IP harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G105 (VIN 6) | The center rear of the engine, on the intake manifold | -- | --
G203 | The junction-block case ground, under the left side of the IP | -- | --
S222 | The IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views in Wiring Systems | --
S235 | The IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S236 | The IP harness, approximately 8 cm (3.125 in) from the C3 breakout of the IP cluster assembly connector | Harness Routing Views in Wiring Systems | --
S237 | The IP harness, approximately 10 cm (4 in) from the radio-connector breakout | Harness Routing Views in Wiring Systems | --
S240 | The IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views in Wiring Systems | --
S245 | The IP harness, approximately 12 cm (5 in) from the C3 breakout of the I/P cluster assembly connector | Harness Routing Views in Wiring Systems | --
S249 | The IP harness, approximately 1 cm (0.375 in) from the C2 breakout of the IP cluster assembly connector | Harness Routing Views in Wiring Systems | --