For 1990-2009 cars

## Door Adjustment Specifications 2 Door

#### 2-Door Model, Sheet Metal Tolerances

Location | Clearance Gap | Flushness
--- | --- | ---
Important: The following specifications are to be used to ensure the proper clearances and flushness of the doors after body repair procedures are complete.
1: Front Door to Fender | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
2: Front Door to Quarter Panel | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
3: Front Door to Rocker Panel | 5.9 mm (0.23 in) | -6.5 to -4.5 mm (-0.26 to -0.18 in)
4: Rocker Panel to Fender | 2.5 mm (0.10 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
5: Side Window to Windshield | 8.9 mm (0.35 in) | --

## Door Adjustment Specifications 4 Door

#### 4-Door Model, Sheet Metal Tolerances

Location | Clearance Gap | Flushness
--- | --- | ---
Important: The following specifications are to be used to ensure the proper clearances and flushness of the doors after body repair procedures are complete.
1: Front Door to Fender | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
2: Front Door to Rear Door | 5.6 mm (0.22 in) | 0.0 to 1.0 mm (0.00 to 0.04 in)
3: Front Door to Rear Door | 5.0 mm (0.20 in) | 0.0 to 1.0 mm (0.00 to 0.04 in)
4: Front Door to Rocker Panel | 5.9 mm (0.23 in) | -6.5 to -4.5 mm (-0.26 to -0.18 in)
5: Rear Door to Quarter Panel | 5.1 mm (0.20 in) | 0.0 to 1.0 mm (0.00 to 0.04 in)
6: Rocker Panel to Fender | 2.5 mm (0.10 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
7: Side Window to Windshield | 8.9 mm (0.35- in) | --