For 1990-2009 cars

### Removal Procedure

1. Remove the right wheel drive shaft assembly from the vehicle. Refer to Wheel Drive Shaft Replacement .
2. Remove the three bolts from the intermediate shaft bearing arbor (1).
3. Remove the intermediate shaft (2) from the transaxle.
4. Inspect the intermediate shaft (2) and the intermediate shaft bearing for rough operation, excessive wear or damage. For disassembly and inspection procedures, refer to Intermediate Shaft Overhaul .

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the intermediate shaft (2) into the transaxle. Secure with three bolts in the intermediate shaft bearing arbor.

Tighten
Tighten the intermediate shaft bearing arbor bolts to 60 N·m (44 lb ft).

2. Install the right wheel drive shaft assembly to the vehicle. Refer to Wheel Drive Shaft Replacement .