For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Module | Below right side of the IP, attached to evaporator case | HVAC Component Views In HVAC System - Manual | HVAC Connector End Views In HVAC System - Manual
Blower Speed Selector Switch | Center of IP, above radio | Heater Blower Controls Component Views In Heating, Ventilation, and Air Conditioning | --
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views In Engine Electrical | --
Crankshaft Position Sensor | Bottom of the engine, mounted to the engine near the crankshaft pulley | Engine Controls Component Views | Engine Controls Connector End Views
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views In Wiring Systems | Data Link Communications Connector End Views In Wiring Systems
Diode Module | Behind the center IP, taped to the IP harness | Lighting Systems Component Views In Lighting Systems | Engine Controls Connector End ViewsIn Lighting Systems
Distributor | Left side of the engine | -- | --
Duty Check Data Link Connector | Passenger compartment, taped to the harness behind the IP compartment | Data Link Communications Component Views In Wiring Systems | Data Link Communications Connector End Views In Wiring Systems
Early Fuel Evaporation (EFE) Heater | Mounted between the intake manifold and the throttle body | Engine Controls Component Views | --
Engine Coolant Temperature (ECT) Sensor | Left side of the engine, mounted in thermostat housing | Engine Controls Component Views | Engine Controls Connector End Views
Engine Cooling Fan Motor | Left front side of the engine compartment, behind the radiator | -- | Engine Controls Connector End Views
EVAP Canister Purge Valve | Center engine compartment, on the intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
EVAP Canister Vent Solenoid (without ORVR) | Center of engine bulkhead | -- | Engine Controls Connector End Views
EVAP Canister Vent Solenoid (with ORVR) | Top of the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
EVAP Tank Pressure Control Solenoid Valve (Without ORVR) | On engine bulkhead, next to EVAP canister | -- | Engine Controls Connector End Views
EVAP Tank Pressure Control Solenoid Valve (With ORVR) | Top of the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
Exhaust Gas Recirculation Vacuum Solenoid (EGR SV) Valve | Left side of the engine, next to the intake manifold | Engine Controls Component Views | --
Exhaust Gas Recirculation (EGR) Bypass Valve | Left side of the engine, next to the intake manifold | Engine Controls Component Views | --
Fuel Injector | In the engine throttle body | Engine Controls Component Views | --
Fuel Injector Resistor | Left rear side of the engine compartment, attached to the bulkhead | Engine Controls Component Views | --
Fuel Sender Assembly | In the fuel tank | Engine Controls Component Views | Instrument Panel, Gages, and Console Connector End Views In Instrument Panel, Gauges, and Console
Fuel Tank Pressure Sensor | In the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
Fuse Box | Left side of the engine compartment, mounted on Left inner side of the fender, behind the relay box | Power and Grounding Component Views In Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Heated Oxygen Sensor 1 (HO2S1) | Front of the engine in the exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor 2 (HO2S2) | Below vehicle after a three-way catalytic converter (TWC) | Engine Controls Component Views | --
Idle Speed Control (ISC) Motor | Top of engine, mounted to the throttle body | Engine Controls Component Views | --
Ignition Control Module | Left engine compartment on the bulkhead near the strut tower | Engine Controls Component Views | --
Ignition Coil | Left side of the engine compartment, on the bulkhead | Engine Controls Component Views | --
Ignition Switch | Right side of the steering column | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views In Instrument Panel, Gauges, and Console
Intake Air Temperature (IAT) Sensor | Center engine compartment attached to air cleaner (ACL) housing | Engine Controls Component Views | Engine Controls Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views In Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Manifold Absolute Pressure (MAP) Sensor | Right rear engine compartment, on the bulkhead | Engine Controls Component Views | Engine Controls Connector End Views
Noise Suppressor Filter | Left rear engine compartment, taped to the harness, below the ignition control module | Engine Controls Component Views | --
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views | Powertrain Control Module Connector End Views
Rear Defogger Switch | In the IP, left of steering column | -- | Stationary Windows Connector End Views In Stationary Windows
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views In Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Throttle Position (TP) Sensor | Right rear side of the engine, attached to the throttle body | Engine Controls Component Views | --
Turn Signal/Combination Switch | On steering column | -- | Lighting Systems Connector End Views In Lighting Systems
Vehicle Speed Sensor (VSS) (Automatic Transaxle) | Left side of the engine compartment, top of the transaxle | -- | --
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C113 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near the bulkhead | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C201 (14 Cavities) | Main harness to the floor harness, behind the left side of the IP, near junction block | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C203 (13 Cavities) | I/P harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C204 (2 Cavities) (Manual Transaxle) | Main harness to clutch pedal position switch, behind left side of the IP | Harness Routing Views In Wiring Systems | --
C205 (12 Cavities) | IP harness to engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C208 (8 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C211 (6 Cavities) | IP harness to blower speed selector switch jumper, behind the center of the IP | Harness Routing Views In Wiring Systems | --
C300 (2 Cavities) | Floor harness to fuel tank jumper harness, under the rear passenger seat | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C310 (4 Cavities) | Floor harness to fuel tank jumper harness, under rear passenger seat | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
C311 (3 Cavities) | Floor harness to fuel tank jumper harness, under the rear passenger seat | Harness Routing Views In Wiring Systems | Inline Harness Connector End Views In Wiring Systems
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views In Wiring Systems | --
G104 | Center rear side of the engine on the intake manifold | Harness Routing Views In Wiring Systems | --
G105 (VIN 6) | Center rear of engine, on the intake manifold | -- | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G400 (2-Door) | Rear center of luggage compartment | Harness Routing Views In Wiring Systems | --
G400 (4-Door) | Rear center of luggage compartment | Harness Routing Views In Wiring Systems | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views In Wiring Systems | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views In Wiring Systems | --
P300 | Below the right rear passenger seat | Harness Routing Views In Wiring Systems | --
S101 | Main harness, approximately 11 cm (4.5 in) from the brake fluid level switch breakout | Harness Routing Views In Wiring Systems | --
S110 | Main harness, approximately 5 cm (2 in) from the ignition control module connector breakout | -- | --
S111 (VIN 6) | Main harness, approximately 7 cm (2.8 in) from the ignition coil breakout | -- | --
S118 (VIN 6) | Main harness, approximately 28 cm (11.5 in) from the front wiper motor connector breakout | -- | --
S119 | Main harness, approximately 50 cm (20 in) from the front wiper motor connector breakout | Harness Routing Views In Wiring Systems | --
S120 (VIN 6) | Main harness, approximately 6 cm (2.4 in) from the ignition coil connector breakout | -- | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views In Wiring Systems | --
S127 (Manual Transaxle) | Engine harness, at the generator breakout | -- | --
S127 (Automatic Transaxle) | Engine harness, 5 cm (2 in) from the starter breakout | -- | --
S129 (VIN 6) | Engine harness, approximately 14 cm (5.6 in) from the TP sensor breakout | -- | --
S129 (VIN 2) | Engine harness, approximately 2 cm (1 in) from the C113 breakout | -- | --
S130 | Engine harness, approximately 5 cm (2 in) from starter breakout | Harness Routing Views In Wiring Systems | --
S131 | Engine harness, approximately 9 cm (3.6 in) from the generator connector breakout | Harness Routing Views In Wiring Systems | --
S148 | Main harness, approximately 23 cm (9.2 in) from the MAP sensor connector breakout | -- | --
S151 | Main harness, approximately 5 cm (2 in) from the relay box | Harness Routing Views In Wiring Systems | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views In Wiring Systems | --
S153 | Main harness, approximately 13 cm (5.125 in) from the front wiper motor connector breakout | Harness Routing Views In Wiring Systems | --
S156 | Engine harness, approximately 7 cm (3 in) from P202 | Harness Routing Views In Wiring Systems | --
S167 | Engine harness, approximately 14 cm (6 in) from the C113 breakout | Harness Routing Views In Wiring Systems | --
S168 (VIN 6) | Engine harness, approximately 4 cm (2 in) from the C113 breakout | -- | --
S169 (VIN 6) | Engine harness, approximately 4 cm (2 in) from the EGR SV valve breakout | -- | --
S170 (VIN 6) | Engine harness, approximately 11 cm (4.3 in) from P202 | -- | --
S200 (VIN 6) | Main harness, approximately 15 cm (6 in) from the C208 breakout | -- | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S204 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C5 breakout | -- | --
S218 | IP harness, approximately 3 cm (1.19 in) from the IP custer assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S221 | IP harness, approximately 7 cm (3 in) from the IP cluster assembly connector C2 breakout | Harness Routing Views In Wiring Systems | --
S222 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2 ) breakout | Harness Routing Views In Wiring Systems | --
S225 | I/P harness, approximately 2 cm (1 in) from the C200 breakout | Harness Routing Views In Wiring Systems | --
S226 | IP harness, approximately 3 cm (1.19 in)from the IP cluster assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S231 | Main harness, approximately 15 (6 in) cm from P200 | -- | --
S232 | IP harness, approximately 4 cm (2 in) from the C205 breakout | Harness Routing Views In Wiring Systems | --
S233 | IP harness, approximately 8 cm (3.125 in) from the blower motor branch breakout | Harness Routing Views In Wiring Systems | --
S234 | IP harness, approximately 1 cm (.375 in) from the diode module connector breakout | Harness Routing Views In Wiring Systems | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views In Wiring Systems | --
S236 | IP harness, approximately 8 cm (3.125 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S237 | IP harness, approximately 10 cm (4 in) from the radio connector breakout | Harness Routing Views In Wiring Systems | --
S240 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD 2) breakout | Harness Routing Views In Wiring Systems | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S245 | IP harness, approximately 12 cm (5 in) from the I/P cluster assembly connector C3 breakout | Harness Routing Views In Wiring Systems | --
S248 | Engine harness, approximately 4 cm (2 in) from the powertrain control module (PCM) connector C1 breakout | Harness Routing Views In Wiring Systems | --
S252 | IP harness, approximately 4 cm (2 in) from the data link connector - (DLC-OBD 2) breakout | Harness Routing Views In Wiring Systems | --
S256 | Main harness, near the junction block connector C6 breakout |  | --
S257 (VIN 6) | Engine harness, approximately 5 cm (2 in) from P202 | -- | --
S261 (Manual Transaxle) | Engine harness, approximately 4 cm (2 in) from PCM connectors breakout | Harness Routing Views In Wiring Systems | --
S262 | Engine harness, approximately 5 cm (2 in) from P202 | Harness Routing Views In Wiring Systems | --
S263 | Engine harness, approximately 3 cm (1.9 in) from the C205 breakout | Harness Routing Views In Wiring Systems | --
S315 | Fuel tank jumper harness, approximately 10 cm (4 in) from P300 | Harness Routing Views In Wiring Systems | --