For 1990-2009 cars

Causes | Correction
--- | ---
Linings damaged by abusive use | Replace the brake linings.
Damaged vacuum booster | Replace the vacuum booster.
Worn out brake linings | Replace the brake linings.
Uneven brake lining wear | Replace the brake linings.
Incorrect lining material | Replace the brake linings.
Improper rotor surface finish | Refinish the rotor surface or replace the rotor.
Scored rotor | Refinish the rotor surface or replace the rotor.
Improper thickness variation in the rotor | Repair or replace the rotor.
Excessive rotor lateral runout | Repair or replace the rotor.
Loose front or rear brake assembly attachment | Locate and tighten the loose brake components.