For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the wiper/washer system check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Turn the ignition switch to the ON position.
2. Move the front wiper/washer switch lever to the HI position.
3. Backprobe the front wiper motor connector using J 35616-200 from cavity 2 to ground.

Does the test lamp light?

--

Go to Step 4

Go to Step 3

3 | Test for an open in the BLU/RED wire between the combination switch and the front wiper motor. Was an open found? | -- | Go to Step 6 | Go to Step 5
4 | Replace the front wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
5 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in Restraints. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --