For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Set the dome lamp to the DOOR position.
2. Open and close the left front door.

The dome lamp lights when the door is opened and goes out when the door is closed.

Dome Lamps Inoperative with Left Front Door Open

2 | Turn the dome lamp to the ON position and then back to the DOOR position. | The dome lamp lights, then goes out. | Dome Lamps Inoperative
3 |

1. Turn the dome lamp to the OFF position.
2. Open and Close the LH front door.

The dome lamp does not light at all.

Courtesy Lamps Always On

4 | Open and close the deck lid (4 door LSi only) | The luggage compartment lamp lights when the deck lid is open. The lamp goes out when the deck lid is closed. | Cargo Lamp Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.