For 1990-2009 cars

## Rear Compartment Lid Weatherstrip Replacement 2-Door

### Removal Procedure

1. Pull the weatherstrip (1) from the opening pinch-weld flange.
2. Remove the weatherstrip (1) from the vehicle.

### Installation Procedure

1. Apply a thin bead of weatherstrip adhesive GM P/N 12345096, or equivalent, around the perimeter of the weather-strip opening pinch-weld flange.
2. Install the weatherstrip (1) to the opening pinch-weld flange.
3. Press the weatherstrip (1) firmly into place.

## Rear Compartment Lid Weatherstrip Replacement 4-Door

### Removal Procedure

1. Pull the weatherstrip (2) from the opening pinch-weld flange.
2. Remove the weatherstrip (2) from the vehicle.

### Installation Procedure

1. Apply a thin bead of weatherstrip adhesive GM P/N 12345096, or equivalent, around the perimeter of the weatherstrip opening pinch-weld flange.
2. Install the weatherstrip (2) to the opening pinch-weld flange.
3. Press the weatherstrip (2) firmly into place.