For 1990-2009 cars

# Information - August, 2000 Bulletin Summary

Subject: | Information -- August, 2000 Bulletin Summary

Models: | 2001 and Prior Passenger Cars and Trucks

The following list is a summary of all the bulletins that were issued in August, 2000. It is intended to let dealerships quickly review the most current bulletins in order to better service their customers. Dealerships will be receiving this type of summary, published as a bulletin, every month.

Bulletin Title | Vehicles Affected | Bulletin Number
--- | --- | ---
Engine
Revised Diagnostic Information for Diagnostic Trouble Code (DTC) P0400, Exhaust Gas Recirculation System Performance | 1996-1998 Chevrolet Tracker With 1.6L Engine | 00-06-04-027
Engine Oil Level Indicator and Tube Change | 2000 Chevrolet and GMC C/K Pickup Models (Silverado and Sierra) With 4.8L, 5.3L or 6.0L V8 Engine | 00-06-01-015A
Revised Fuel Pressure Operating Range | 2001 Buick LeSabre, Park Avenue, Regal; 2001 Chevrolet Impala, Monte Carlo; 2001 Pontiac Bonneville, Grand Prix With 3.8L Engine | 00-06-04-030
Bang/Slosh From Rear of Vehicle (Install Fuel Tank Insulators) | 2000 Buick Century, Regal; 2000 Chevrolet Impala, Monte Carlo | 00-06-04-028
Transmissions
Slips, Harsh Upshift or Garage Shifts, Launch Shudders, Flares, Erratic Shifts and Intermittent Concerns, DTC P1811 or P0748 Set (Replace Pressure Control Solenoid Valve Assembly) | 1999-2000 Buick LeSabre, Park Avenue/Ultra, Regal, Riviera; 1999 Chevrolet Lumina, Monte Carlo, Venture; 1999 Oldsmobile Eighty-Eight, Intrigue, Silhouette; 1999 Pontiac Bonneville, Grand Prix, Montana With Hydra-Matic 4T65-E and 3.4L, 3.5L or 3.8L Engine | 00-07-30-002A
Steering, Suspension , Tires and Wheels
Power Steering System Whistle (Replace Power Steering Gear (Rack and Pinion) Assembly) | 2000 Chevrolet and GMC C1500 Pickup Models (Silverado and Sierra) | 00-02-32-002
Steering Column Ignition Lock Cylinder Binds (Replace Ignition Lock Cylinder Case Assembly) | 2000 Cadillac DeVille | 00-02-35-006
Procedure to Disable Illumination of Service Indicator AFTER the Installation of Passive Struts/Shocks | 1992-1994 Buick Skylark; 1993-1996 Buick Park Avenue; 1989-1992 Cadillac Allante; 1991-1993 Cadillac Eldorado, Seville; 1991-1995 Cadillac DeVille; 1991-1995 Oldsmobile Ninety Eight; 1992-1993 Oldsmobile Achieva; 1994-1999 Pontiac Bonneville | 00-03-11-001A
Body and Accessories
Onboard Rear Seat Entertainment Package | 2000 Cadillac Escalade | 00-08-44-007
Revised Assist Step Installation Procedure | 2000 Chevrolet and GMC C/K 1-2 Utility Trucks (Suburban, Tahoe, Yukon, Yukon XL) | 00-08-61-001
Power Antenna Not Working Properly or is Completely Inoperative (Replace Antenna O-Ring Assembly/Cap Nut & Clean Mast) | 2000 Chevrolet Camaro, Corvette; 2000 Pontiac Firebird; 2000 Chevrolet and GMC G Van | 00-08-44-006A
Tail Lamp Wiring Harness Routing | 2000 Chevrolet Monte Carlo | 00-08-42-004
Revised Front and Rear Door Trim Panel Replacement Procedures | 2000 Buick LeSabre | 00-08-64-005A
Broken Mounting Tabs on Console Rear Seat Cupholder (Replace Rear Console Housing) | 1999-2000 Pontiac Grand Am | 00-08-49-008
Inoperative Power Sunroof in Open/Closed Position (Replace Sunroof Control Module Assembly) | 2000-2001 Buick Park Avenue/Ultra | 00-08-67-003
Front and Rear Side Door Front Upper Trim Panel (Shark Fin) Loose Fit/Gap (Install Retainer) | 2001 Oldsmobile Aurora | 00-08-64-001A
General Information
August, 2000 Labor Time Guide Updates | 1996-2001 Passenger Cars and Trucks | 00-00-89-017
General Motors Tire Warranty | 1996-2001 Passenger Cars and Light Duty Trucks (Except Saturn Models) | 00-03-10-003
Brakes
Electronic Brake Control Module (EBCM) Replacement | 1990-2000 Chevrolet and GMC Medium Duty Conventional T-Series Tilt Cab and B7 School Bus Models With 7.4L Engine and Hydraulic ABS Brakes | 00-05-25-002
HVAC
Air Conditioning Not Cold Enough/Inoperative (Replace O-Rings/Recharge System) | 1999-2000 Chevrolet Tracker | 00-01-38-002A
Delphi-Harrison and Denso A/C Compressor Usage | 2000-2001 Chevrolet and GMC C/K Pickup Models With 4.8L, 5.3L or 6.0L Gen III Gas Engines | 00-01-37-003
Essential Tool J43600 ACR 2000 | 1993-2001 Passenger Cars and Trucks (Except Medium Duty Trucks) | 00-01-38-006