For 1990-2009 cars

### Removal Procedure

1. Remove two screws and disconnect the electrical connectors and then remove the junction block from the instrument panel.
2. Disconnect the EBCM electrical connectors.
3. Remove the three bolts (1) and remove the EBCM (2) from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the EBCM (2) to the vehicle; secure with three bolts (1).

Tighten
Tighten the attaching bolts to 8 N·m (71 lb in).

2. Connect the EBCM electrical connectors.
3. Install the junction block to the instrument panel and reconnect all electrical connectors.
4. Secure junction block with two screws.
5. Perform the A Diagnostic System Check - ABS