For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the vehicle:

• | The plastic retainer that secures the front bumper valance panel

• | The three screws (2) that secure the front bumper valance panel

• | The front bumper valance panel (1)

### Installation Procedure

1. Install the front bumper valance panel (1) to the vehicle. Secure the panel with the following components:

• | The plastic retainer

• | The three screws (2)

2. Lower the vehicle.