For 1990-2009 cars

## Rear Turn Signal Lamp Bulb Replacement 2 Door

### Removal Procedure

1. Remove the 2 screws that retain the tail lamp (5).
2. Remove the tail lamp (5) from the vehicle by pulling upward and rearward.
3. Remove the turn signal lamp bulb socket from the tail lamp (5).
4. Remove the turn signal lamp bulb (2) from the socket.

### Installation Procedure

1. Install the turn signal lamp bulb (2) to the turn signal lamp bulb socket.
2. Install the socket to the tail lamp (5).
3. Install the tail lamp (5) to the vehicle. Secure the lamp with the 2 screws.

## Rear Turn Signal Lamp Bulb Replacement 4 Door

### Removal Procedure

1. Open the rear compartment lid.
2. Reposition the rear compartment side trim in order to access the nut that retains the tail lamp.
3. Remove the nut that retains the tail lamp (1).
4. Remove the 2 screws that retain the tail lamp (1).
5. Remove the tail lamp (1) from the body in order to access the turn signal lamp bulb socket.
6. Remove the turn signal lamp bulb socket from the tail lamp (1).
7. Remove the turn signal lamp bulb (4) from the socket.

### Installation Procedure

1. Install the turn signal lamp bulb (4) to the turn signal lamp bulb socket.
2. Install the socket to the tail lamp (1).
3. Install the tail lamp (1) to the vehicle. Secure the lamp with 2 screws and with the nut.
4. Position the rear compartment side trim back to the original position.
5. Close the rear compartment lid.