For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 | Disconnect the connector of the left door jamb switch. Does the warning alarm continue to sound? | -- | Go to Step 4 | Go to Step 3
3 | Replace the left door jamb switch. Is the repair complete? | -- | Go to Audible Warnings System Check | --
4 | Test for a short to ground in the BLK/BLU wire between cavity 6 and the connector of the left front door jamb switch. Was a short to ground condition found? | -- | Go to Step 5 | Go to Step 6
5 | Repair the short to ground in the BLK/BLU wire between cavity 6 and the connector of the left front door jamb switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
6 | Replace the audio alarm module. Refer to Audio Alarm Module Replacement . Is the repair complete? | -- | Go to Audible Warnings System Check | --