For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Slide out the hood latch release cable sideways in order to release the cable from the hood latch assembly.
3. Remove the following components:

• | 6 screws

• | 5 plastic clips

• | The left wheelhouse panel

4. Remove 2 screws. Pull the hood latch release lever and the cable from the instrument panel.

### Installation Procedure

1. Install the hood release cable through the following components to the hood latch assembly:

• | The instrument panel

• | The cowl

• | The inner fender

2. Connect the cable to the hood latch assembly.
3. Install the hood latch release lever to the knee bolster. Secure the lever with the 2 screws.
4. Install the left front wheelhouse panel. Secure the wheelhouse with the following components:

• | 6 screws

• | 5 plastic clips