For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the front side door trim (1):

• | 1 screw

• | The inside handle bezel (2)

2. Remove 2 caps from the front door pull handle.
3. Remove the following components from the front door:

• | The 2 screws

• | The front door pull handle

4. Remove the outside rearview mirror garnish (8) from the door (1).
5. Remove the window-regulator handle (1) by using a cloth in order to pull off the snap ring.
6. Gently pry the door trim (1) from the door by disengaging the retainers.
7. Disconnect the electrical connectors from the power window or from the power door switch, if necessary.
8. Remove the door trim (1) from the vehicle.

### Installation Procedure

1. Connect the electrical connectors to the power window or to the power door switch, if necessary.
2. Position the front side door trim (1) to the front door. Press the retainers into place.
3. Install the snap ring to the window-regulator handle (3).
4. Set the regulator handle (3) at a 45-degree angle when the front door window is completely closed.
5. Install the regulator handle (3) to the door.
6. Install the front door pull handle to the door. Secure the handle with the 2 screws.
7. Install the caps to the pull handle.
8. Install the outside rearview mirror garnish (8) to the door (1).
9. Install the inside handle bezel (2) to the door trim (1). Secure the bezel with the screw.