For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Audio Alarm Module | Left side of the lower IP, left of Steering column | Audible Warnings Component Views | Audible Warnings Connector End Views
Engine Coolant Temperature (ECT) Sensor | Left side of the engine, mounted in thermostat housing | Engine Controls Component Views in Engine Controls,1.0L,1.3L | Engine Controls Connector End Views in Engine Controls,1.0L,1.3L
Fuel Sender Assembly | In the fuel tank | Engine Controls Component Views in Engine Controls,1.0L,1.3L | Instrument Panel, Gages, and Console Connector End Views
Ignition Key Warning Switch | Right side of the steering column, on the ignition switch cylinder | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Oil Pressure Switch | Front of the engine, behind the exhaust manifold | -- | --
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views in Engine Controls,1.0L,1.3L | Powertrain Control Module Connector End Views in Engine Controls,1.0L,1.3L
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Turn Signal/Combination Switch | On steering column | -- | Lighting Systems Connector End Views in Lighting Systems
Vehicle Speed Sensor (VSS) (Automatic Transaxle) | Left side of the engine compartment, top of the transaxle | -- | --
C113 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (13 Cavities) | IP harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 (12 Cavities) | IP harness to engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C300 (2 Cavities) | Floor harness to fuel tank jumper harness, under the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C310 (4 Cavities) | Floor harness to fuel tank jumper harness, under rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G104 | Center rear side of the engine on the intake manifold | Harness Routing Views in Wiring Systems | --
G105 (VIN 6) | Center rear of engine, on the intake manifold | -- | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G400 (2-Door) | Rear center of luggage compartment | Harness Routing Views in Wiring Systems in Wiring Systems | --
(4-Door) | Rear center of luggage compartment | Harness Routing Views | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views in Wiring Systems | --
P300 | Below the right rear passenger seat | Harness Routing Views in Wiring Systems | --
S111 (VIN 6) | Main harness, approximately 7 cm (2.8 in) from the ignition coil breakout | -- | --
S167 | Engine harness, approximately 14 cm (6 in) from the C113 breakout | Harness Routing Views in Wiring Systems | --
S200 (VIN 6) | Main harness, approximately 15 cm (6 in) from the C208 breakout | -- | --
S204 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C5 breakout | -- | --
S218 | IP harness, approximately 3 cm (1.19 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S219 | IP Harness, approximately 3 cm (1.19 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S226 | IP harness, approximately 3 cm (1.19 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S245 | IP harness, approximately 12 cm (5 in) from the I/P cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S256 | Main harness, near the junction block connector C6 breakout | -- | --
S301 (2-Door) | Floor harness, approximately 20 cm (8 in) from the center console branch breakout | Harness Routing Views in Wiring Systems | --
S311 (4-Door) | Floor harness, approximately 10 cm (4 in) from the C400 breakout | Harness Routing Views in Wiring Systems | --
S315 | Fuel tank jumper harness, approximately 10 cm (4 in) from P300 | Harness Routing Views in Wiring Systems | --
S402 (2-Door) | Floor harness, approximately 5 cm (2 in) from the left rear combination lamp connector breakout | -- | --
S403 (2-Door) | Floor Harness, approximately 5 cm (2 in) from G400 breakout | -- | --
S406 (4-Door) | Floor harness, approximately 10 cm (4 in) from the left rear combination lamp connector breakout | -- | --
S407 (4-Door) | Floor harness, approximately 20 cm (8 in) from the left rear combination lamp connector breakout | -- | --
S408 (4-Door) | Floor harness, approximately 5 cm (2 in) from the C400 breakout | -- | --