For 1990-2009 cars

### Removal Procedure

1. Remove the transaxle from the engine. Refer to Transaxle Assembly Removal in Manual Transmission.
2. Remove the pressure plate assembly and the clutch disc. Refer to Clutch Pilot Bearing Replacement in Clutch.
3. Replace the flywheel if any of the following conditions exist on the ring gear or on the surface that contacts the clutch disc:

• | Cracks

• | Excessive wear

• | Damage

4. Mark the flywheel-to-engine position.
5. Remove the flywheel retaining bolts (1) and the flywheel from the crankshaft.
6. Remove the clutch pilot bushing from the flywheel.
7. Clean all grease and dirt from the flywheel outer surfaces.

### Installation Procedure

1. Install the clutch pilot bushing into the flywheel.
2. Align the flywheel-to-engine marks. Install the flywheel to the crankshaft.

Notice: Apply the proper amount of the sealant to the fastener when assembling this component. Excessive use of the sealant can prohibit the component from being assembled properly or allow the fastener to loosen. A component or fastener that is not assembled properly can loosen or fall off leading to extensive engine damage.

3. Apply GM P/N 12345493 or equivalent, to the flywheel retaining bolt threads.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the flywheel retaining bolts to the flywheel.

Tighten
Tighten the flywheel retaining bolts to 75 N·m (55 lb ft.)

5. Install the pressure plate assembly and the clutch disc. Refer to Clutch Pilot Bearing Replacement in Clutch.
6. Install the transaxle to the engine. Refer to Transaxle Assembly Installation in Manual Transmission.